1. PRODUCT AND COMPANY IDENTIFICATION
Product information
Trade name	:	RAID MAX® WASP & HORNET FOAM BUG KILLER (REG NO 25303 P.C.P. ACT)
	
Use of the Substance/Mixture	:	Insecticide
	
Company	:	S.C. Johnson and Son, Limited
1 Webster Street
Brantford   ON   N3T 5R1
  	
Emergency telephone number	:	 24 Hour Transport & Medical Emergency Phone (866) 231-5406
24 Hour International Emergency Phone (952) 852-4647
24 Hour Canadian Transport Emergency Phone (CANUTEC) (613) 996-6666

2. HAZARDS IDENTIFICATION
Emergency Overview Appearance / Odor	:	off-white / aerosol / characteristic	

Immediate Concerns
	:	Caution
Avoid contact with skin, eyes and clothing.
Keep away from heat, sparks and flame.
Do not puncture or incinerate.
Do not store at temperatures above 120 Deg. F (50 Deg C), as container may burst.
Avoid breathing vapors, mist or gas.
Contents under pressure.
Harmful if absorbed through skin.

Potential Health Effects
Exposure routes	:	Eye, Skin, Inhalation, Ingestion. 
	
Eyes	:	May cause: 
Mild eye irritation 
	
Skin	:	Harmful if absorbed through skin. 
Moderate skin irritant 
Prolonged or repeated contact may dry skin and cause irritation. 
	
Inhalation	:	Excessive exposures may affect human health, as follows: 
Inhalation may cause central nervous system effects. 
May be harmful if inhaled. 
	
Ingestion	:	Causes headache, drowsiness or other effects to the central nervous system. 
Aspiration hazard if swallowed - can enter lungs and cause damage. 
	
Aggravated Medical Condition	:	None known. 

3. COMPOSITION/INFORMATION ON INGREDIENTS
Hazardous chemicals present at or above reportable levels as defined by OSHA 29 CFR 1910.1200 or the Canadian Controlled Products Regulations are listed in this table:

Chemical Name	CAS-No.	Weight percent	
Ethyl alcohol	64-17-5	 10.00 - 30.00	
Isobutane	75-28-5	 5.00 - 10.00	
Propane	74-98-6	 5.00 - 10.00	
n-Octyl bicycloheptene dicarboximide	113-48-4	 0.10 - 1.00	
Permethrin	52645-53-1	 0.10 - 1.00	
D-trans allethrin	584-79-2	 0.0001 - 0.10	

For additional information on product ingredients, see www.whatsinsidescjohnson.com.

4. FIRST AID MEASURES
Eye contact	:	Flush immediately with plenty of water for at least 15 to 20 minutes. Remove contact lenses. Get medical attention if irritation develops and persists. 
	
Skin contact	:	Flush immediately with plenty of water for at least 15 to 20 minutes. Get medical attention immediately. Remove contaminated clothing and shoes. Wash clothing before reuse. Thoroughly clean shoes before reuse. 
	
Inhalation	:	Remove to fresh air. If breathing is affected, get medical attention. 
	
Ingestion	:	If swallowed, DO NOT induce vomiting unless directed to do so by medical personnel. Never give anything by mouth to an unconscious person. Get medical attention immediately. 

5. FIREFIGHTING MEASURES
Suitable extinguishing media	:	Use water spray, alcohol-resistant foam, dry chemical or carbon dioxide.	

Specific hazards during firefighting	:	Burns with colourless flame. Aerosol Product - Containers may rocket or explode in heat of fire. Container may melt and leak in heat of fire. Do not allow run-off from fire fighting to enter drains or water courses. 	

Further information	:	Fight fire from maximum distance or protected area. Cool and use caution when approaching or handling fire-exposed containers. Wear full protective clothing and positive pressure self-contained breathing apparatus. In case of fire and/or explosion do not breathe fumes. 	

Flash point	:	< -7 °C
< 19.4 °F
Method: Tag Closed Cup  (TCC)
Note: Propellant
	
Lower explosion limit	:	Note: no data available
	
Upper explosion limit	:	Note: no data available
	
NFPA Classification	:	NFPA Level 1 Aerosol              	

6. ACCIDENTAL RELEASE MEASURES
Personal precautions	:	Remove all sources of ignition.
Wear personal protective equipment.
	
Environmental precautions	:	Do not flush into surface water or sanitary sewer system.
Use appropriate containment to avoid environmental contamination.
Outside of normal use, avoid release to the environment.
	
Methods for cleaning up	:	Soak up with inert absorbent material.
If damage occurs to aerosol can:
Contain spillage, soak up with non-combustible absorbent material, (e.g. sand, earth, diatomaceous earth, vermiculite) and transfer to a container for disposal according to local / national regulations (see section 13).
Sweep up and shovel into suitable containers for disposal.
Use only non-sparking equipment.
Dike large spills.
Clean residue from spill site.

7. HANDLING AND STORAGE
Handling
Advice on safe handling	:	Do not puncture or incinerate.
Do not enter places where used or stored until adequately ventilated.
Avoid breathing vapors, mist or gas.
Do not spray toward face.
Do not use in areas without adequate ventilation.
Use only as directed.
KEEP OUT OF REACH OF CHILDREN AND PETS.
Smoking, eating and drinking should be prohibited in the application area.
	
Advice on protection against fire and explosion	:	Keep away from heat and sources of ignition.

Storage
Requirements for storage areas and containers	:	Keep away from food, drink and animal feedingstuffs.
Do not store at temperatures above 120 Deg. F (50 Deg C), as container may burst.
Keep in a dry, cool and well-ventilated place.

8. EXPOSURE CONTROLS/PERSONAL PROTECTION
Occupational Exposure Limits
Components	CAS-No.	mg/m3
 	ppm 
	Non-standard units	Basis	
Ethyl alcohol	64-17-5	-
1,000 ppm
	-
	ACGIH STEL

Isobutane	75-28-5	-
1,000 ppm
	-
	ACGIH TWA

Propane	74-98-6	-
1,000 ppm
	-
	ACGIH TWA

Personal protective equipment
Respiratory protection
			
Industrial setting	:	Substantial amounts of mist/vapors can be controlled with local exhaust ventilation or respiratory protection.
 Do not spray in enclosed areas.

Household setting	:	Use only with adequate ventilation.	
	
Hand protection
	:	Rubber gloves
	
Eye protection
		
Industrial setting	:	If prolonged or repeated contact is possible:
Safety glasses with side-shields
	
Household setting	:	Avoid contact with eyes.
	
Skin and body protection
:	No special requirements.
	
Hygiene measures	:	Handle in accordance with good industrial hygiene and safety practice. Wash thoroughly after handling. Smoking, eating and drinking should be prohibited in the application area. 

9. PHYSICAL AND CHEMICAL PROPERTIES
Form	:	aerosol
	
Color	:	off-white
	
Odor	:	characteristic
	
pH 	:	8.6 - 9.5
	
Melting point	:	no data available
	
Boiling point	:	78 - 100 °C
	
Freezing point	:	no data available
	
Flash point	:	< -7 °C
< 19.4 °F
Method: Tag Closed Cup  (TCC)
Propellant
	
Evaporation rate	:	no data available
	
Autoignition temperature 	:	no data available
	
Lower explosion limit	:	no data available
	
Upper explosion limit	:	no data available
	
Vapour pressure	:	estimated86.66 hPa
	
Density	:	0.88 - 0.92 g/cm3
	
Water solubility	:	negligible
	
Partition coefficient: n-octanol/water	:	
no data available

10. STABILITY AND REACTIVITY
Conditions to avoid	:	Heat, flames and sparks.
  	
Materials to avoid	:	Strong acids
Do not mix with oxidizing agents.
	
Hazardous decomposition products	:	Thermal decomposition can lead to release of irritating gases and vapours.

Hazardous reactions	:	Stable under recommended storage conditions.

11. TOXICOLOGICAL INFORMATION
Acute oral toxicity	:	LD50
estimated
500 - 5,000 mg/kg

Acute inhalation toxicity	:	no data available

Acute dermal toxicity	:	no data available

Chronic effects
Carcinogenicity	:	None Anticipated	

Mutagenicity	:	None Anticipated	

Reproductive effects	:	None Anticipated

Teratogenicity	:	None Anticipated

Sensitisation	:	no data available	

12. ECOLOGICAL INFORMATION
Ecotoxicity effects	:	Harmful to aquatic organisms, may cause long-term adverse effects in the aquatic environment.	

13. DISPOSAL CONSIDERATIONS
		PESTICIDAL WASTE:
Observe all applicable Federal, Provincial and State regulations and Local/Municipal ordinances regarding disposal.
Consumer may discard empty container in trash, or recycle where facilities exist.

14. TRANSPORT INFORMATION
Land transport
•	U.S. DOT and Canadian TDG Surface Transportation:
Proper shipping name	UN 1950 AEROSOLS, Flammable, 2.1	
Class:	2.1	
UN number	1950	
Packaging group:None. 
Note:	SC Johnson ships this product as "Limited Quantity" when the container quantity value is 1 Liter or less.	

Sea transport
•	IMDG:
Proper shipping name	UN 1950 AEROSOLS, Flammable, 2.1	
Class:	2	
UN number:	1950	
Packaging group:	None.  	
EmS:F-D, S-U	
Note:	SC Johnson ships this product as "Limited Quantity" when the container quantity value is 1 Liter or less.	

Air transport
•	ICAO/IATA:
Proper shipping name	UN 1950 AEROSOLS, Flammable, 2.1
Class:	2.1	
UN/ID No.:	UN 1950	
Packaging group:	None.	
Note:	SC Johnson typically does not ship products via air, therefore it has not been determined if the product container meets current IATA/ICAO package criteria. Refer to IATA/ICAO Dangerous Goods Regulations for detailed instructions when shipping this item by air.	

15. REGULATORY INFORMATION
Notification status	:	All ingredients of this product comply with the New Substances Notification requirements under the Canadian Environmental Protection Act (CEPA).
	
Canada Regulations	:	This product has been classified in accordance with hazard criteria of the Controlled Products Regulations and the MSDS contains all the information required by the Controlled Products Regulations.	

16. OTHER INFORMATION
	HMIS Ratings 
Health	2
	
Flammability	4	
Reactivity	0

NFPA Ratings 
Health	2
	
Fire	4
	
Reactivity	0
	
Special	-

Further information
This document has been prepared using data from sources considered to be technically reliable. It does not constitute a warranty, expressed or implied, as to the accuracy of the information contained herein. Actual conditions of use are beyond the seller's control. User is responsible to evaluate all available information when using product for any particular use and to comply with all Federal, State, Provincial and Local laws and regulations.

Prepared by:	SC Johnson Global Safety Assessment & Regulatory Affairs (GSARA)